{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":27,"n_cols":7,"rows_kept":27,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ACQ-D / AZQS-B(8)V1"]
[]
[]
[]
[]
["","","","","ACQ71DV1 / AZQS71B2V1B","ACQ100DV1 / AZQS100B8V1B","ACQ140DV1 / AZQS140B8V1B"]
["Cooling capacity","Nom.","","kW","6.8","9.5","13.0"]
["Space cooling","SEER","","","5.70","5.50"]
["","Annual energy consumption","","kWh/a","418","605"]
["","Capacity","Pdesign","kW","6.80","9.50"]
["","Energy efficiency class","","","A+","A"]
["Space heating (Average climate)","Capacity","Pdesign","kW","6.33","7.60"]
["","SCOP/A","","","4.00","3.85"]
["","Energy efficiency class","","","A","A"]
["","Annual energy consumption","","kWh/a","2,216","2,764"]
["Nominal efficiency","EER","","","3.31","3.21","3.21"]
["","Annual energy consumption","","kWh","1,025","1,480","2,025"]
["","COP","","","3.61","3.61","3.61"]
["","Energy labeling Directive","Cooling","","A","A","A"]
["","","Heating","","A","A","A"]
["Heating capacity","Nom.","","kW","7.50","10.80","15.5"]
["Notes","","","","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only"]
["","","","","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load"]
["","","","","","(3) - PED: assembly = category l : excluded from scope of PED due to article 1, item 3.6 of 97/23/EC","(3) - PED: assembly = category l : excluded from scope of PED due to article 1, item 3.6 of 97/23/EC"]
["","","","","","(4) - Minimum Ssc (=Short-circuit power) value: Equipment complying with EN 61000-3-2","(4) - Minimum Ssc (=Short-circuit power) value: Equipment complying with EN 61000-3-2"]
["","","","","","(5) - See separate drawing for electrical data","(5) - See separate drawing for electrical data"]
["","","","","","(6) - Contains fluorinated greenhouse gases","(6) - Contains fluorinated greenhouse gases"]