{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":89,"n_cols":9,"rows_kept":89,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ACQ-D"]
[]
[]
[]
[]
["","","","","","ACQ71DV1","ACQ100DV1","ACQ125DV1","ACQ140DV1"]
["Sound pressure level","Heating","","High","dBA","","44","","47"]
["","","","Nom.","dBA","","41","","44"]
["","","","Silent operation","dBA","","36","","41"]
["","","","Low","dBA","","38","","43"]
["","Cooling","","Silent operation","dBA","","36","","41"]
["","","","Low","dBA","","38","","43"]
["","","","High","dBA","","44","","47"]
["","","","Nom.","dBA","","41","","44"]
["Standard Accessories","Installation manual","","","","Installation manual","Installation manual","Installation manual","Installation manual"]
["","Operation manual","","","","Operation manual","Operation manual","Operation manual","Operation manual"]
["","Screws","","","","Screws","Screws","Screws","Screws"]
["","Washer","","","","Washer","Washer","Washer","Washer"]
["","Wireless remote control","","","","Wireless remote control","Wireless remote control","Wireless remote control","Wireless remote control"]
["","Cover lock grill","","","","Cover lock grill","Cover lock grill","Cover lock grill","Cover lock grill"]
["","Battery","","","","Battery","Battery","Battery","Battery"]
["Control systems","Wired remote control","","","","","ARCWB","","ARCWB"]
["","Infrared remote control","","","","","ARCWLA","","ARCWLA"]
["Piping connections","Liquid","","OD","mm","","9.52","","9.52"]
["","Gas","","OD","mm","","15.88","","15.88"]
["","Drain","","","","","19.05","","19.05"]
["Power input","Cooling","","Nom.","kW","","0.094","","0.137"]
["","Heating","","Nom.","kW","","0.094","","0.137"]
["Sound power level","Cooling","","","dBA","","56","","60"]
["","Heating","","","dBA","","56","","60"]
["Dimensions","Unit","","Width","mm","","820","","820"]
["","","","Depth","mm","","820","","820"]
["","","","Height","mm","","300","","300"]
["Casing","Material","","","","","Galvanised steel","","Galvanised steel"]
["Weight","Unit","","","kg","","39","","39"]
["Fan","Air flow rate","Heating","High","m³/min","","29.2","","34.0"]
["","","","Low","m³/min","","21.0","","26.3"]
["","","","Nom.","m³/min","","24.4","","29.2"]
["","","Cooling","Low","m³/min","","21.0","","26.3"]
["","","","Nom.","m³/min","","24.4","","29.2"]
["","","","High","m³/min","","29.2","","34.0"]
["","","","Silent operation","m³/min","","17.6","","22.1"]
["","","Cooling","Silent operation","m³/min","","17.6","","22.1"]
["Decoration panel","Weight","","","kg","","4","","4"]
["","Dimensions","","Height","mm","","82","","82"]
["","","","Depth","mm","","990","","990"]
["","","","Width","mm","","990","","990"]
["","Colour","","","","","White","","White"]
["Power supply","Phase","","","","","1~","","1~"]
["","Name","","","","","V1","","V1"]
["","Frequency","","","Hz","","50","","50"]
["","Voltage","","","V","","220-240","","220-240"]
["Fan","Air flow rate","Heating","Silent operation","m³/min","15","","22.1"]
["Power input","Heating","","Nom.","kW","0.067","","0.137"]
["","Cooling","","Nom.","kW","0.067","","0.137"]
["Fan","Air flow rate","Cooling","Silent operation","m³/min","15","","22.1"]
["Casing","Material","","","","Galvanised steel","","Galvanised steel"]
["Dimensions","Unit","","Height","mm","265","","300"]
["","","","Width","mm","820","","820"]
["","","","Depth","mm","820","","820"]
["Weight","Unit","","","kg","31","","39"]
["Fan","Air flow rate","Cooling","High","m³/min","24.4","","34"]
["","","","Nom.","m³/min","20.5","","29.2"]
["","","","Low","m³/min","17.6","","26.3"]
["","","Heating","High","m³/min","24.4","","34"]
["","","","Nom.","m³/min","20.5","","29.2"]
["","","","Low","m³/min","17.6","","26.3"]
["Sound power level","Cooling","","","dBA","54","","60"]
["","Heating","","","dBA","54","","60"]
["Sound pressure level","Cooling","","High","dBA","41","","47"]
["","","","Nom.","dBA","38","","44"]
["","","","Low","dBA","35","","43"]
["","","","Silent operation","dBA","32","","41"]
["","Heating","","High","dBA","41","","47"]
["","","","Nom.","dBA","38","","44"]
["","","","Low","dBA","35","","43"]
["","","","Silent operation","dBA","32","","41"]
["Piping connections","Liquid","","OD","mm","9.52","","9.52"]
["","Gas","","OD","mm","15.88","","15.88"]
["","Drain","","","","19.05","","19.05"]
["Decoration panel","Dimensions","","Height","mm","82","","82"]
["","","","Width","mm","990","","990"]
["","","","Depth","mm","990","","990"]
["","Weight","","","kg","4","","4"]
["Control systems","Infrared remote control","","","","ARCWLA","","ARCWLA"]
["","Wired remote control","","","","ARCWB","","ARCWB"]
["Power supply","Phase","","","","1~","","1~"]
["","Frequency","","","Hz","50","","50"]
["","Voltage","","","V","220-240","","220-240"]