{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":27,"n_cols":8,"rows_kept":27,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","AHQ-C / AZQS-B(8)V1 UK"]
[]
[]
[]
[]
["","","","","AHQ71CV1 / AZQS71B2V1B UK","AHQ100CV1 / AZQS100B8V1B UK","AHQ125CV1 / AZQS125B8V1B UK","AHQ140CV1 / AZQS140B8V1B UK"]
["Cooling capacity","Nom.","","kW","6.8","9.5","12.1","13.0"]
["Space cooling","SEER","","","4.65","4.60"]
["","Annual energy consumption","","kWh/a","511.85","723"]
["","Capacity","Pdesign","kW","6.80","9.50"]
["","Energy efficiency class","","","B","B"]
["Space heating (Average climate)","Capacity","Pdesign","kW","6.33","7.60"]
["","SCOP/A","","","3.80","3.80"]
["","Energy efficiency class","","","A","A"]
["","Annual energy consumption","","kWh/a","2,332.26","2,800"]
["Nominal efficiency","EER","","","3.03","2.62","2.63","3.01"]
["","Annual energy consumption","","kWh","1,120","1,810","2,300","2,159"]
["","COP","","","3.05","3.41","3.61","3.41"]
["","Energy labeling Directive","Cooling","","B","D","D","B"]
["","","Heating","","D","B","A","B"]
["Heating capacity","Nom.","","kW","7.5","10.8","13.5","15.5"]
["Notes","","","","(1) - Annual energy consumption is according to Energy labeling directive 2002/31/EC","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only"]
["","","","","(2) - SEER and SCOP are according to EN 14825","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load"]
["","","","","(3) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(3) - PED: assembly = category l : excluded from scope of PED due to article 1, item 3.6 of 97/23/EC","(3) - PED: assembly = category l : excluded from scope of PED due to article 1, item 3.6 of 97/23/EC","(3) - PED: assembly = category l : excluded from scope of PED due to article 1, item 3.6 of 97/23/EC"]
["","","","","","(4) - Minimum Ssc (=Short-circuit power) value: Equipment complying with EN 61000-3-2","(4) - Minimum Ssc (=Short-circuit power) value: Equipment complying with EN 61000-3-2","(4) - Minimum Ssc (=Short-circuit power) value: Equipment complying with EN 61000-3-2"]
["","","","","","(5) - See separate drawing for electrical data","(5) - See separate drawing for electrical data","(5) - See separate drawing for electrical data"]
["","","","","","(6) - Contains fluorinated greenhouse gases","(6) - Contains fluorinated greenhouse gases","(6) - Contains fluorinated greenhouse gases"]