{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":68,"n_cols":8,"rows_kept":68,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAHG-G"]
[]
[]
[]
[]
["","","","","FCAHG71GVEB","FCAHG100GVEB","FCAHG125GVEB","FCAHG140GVEB"]
["Sound pressure level","Heating","High","dBA","36","44","45","45"]
["","","Medium","dBA","33","39","40","41"]
["","","Low","dBA","29","33","35","37"]
["","Cooling","Medium","dBA","33","39","40","41"]
["","","Low","dBA","29","33","35","37"]
["","","High","dBA","36","44","45","45"]
["Standard Accessories","Operation manual","","","1","1","1","1"]
["","Installation manual","","","1","1","1","1"]
["","Drain hose","","","1","1","1","1"]
["","Clamp for drain hose","","","1","1","1","1"]
["","Washer for hanger bracket","","","8","8","8","8"]
["","Screws","","","4","4","4","4"]
["","Installation guide","","","1","1","1","1"]
["","Insulation for fitting","","","2","2","2","2"]
["","Sealing pads","","","4","4","4","4"]
["","Drain sealing pad","","","1","1","1","1"]
["","Clamps","","","1","1","1","1"]
["Control systems","Wired remote control","","","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7"]
["","Infrared remote control","","","BRC7FA532F","BRC7FA532F","BRC7FA532F","BRC7FA532F"]
["Cooling capacity","Total capacity","Nom.","kW","","","12.10","13.40"]
["Piping connections","Liquid","OD","mm","9.52","9.52","9.52","9.52"]
["","Gas","OD","mm","15.90","15.90","15.90","15.90"]
["","Drain","","","VP25 (I.D. 25/O.D. 32)","VP25 (I.D. 25/O.D. 32)","VP25 (I.D. 25/O.D. 32)","VP25 (I.D. 25/O.D. 32)"]
["Decoration panel 4","Dimensions","Depth","mm","50","50","50","50"]
["","","Width","mm","950","950","950","950"]
["","","Height","mm","950","950","950","950"]
["","Model","","","BYCQ140D7GFW1","BYCQ140D7GFW1","BYCQ140D7GFW1","BYCQ140D7GFW1"]
["","Colour","","","FRESH WHITE","FRESH WHITE","FRESH WHITE","FRESH WHITE"]
["","Weight","","kg","10.3","10.3","10.3","10.3"]
["Sound power level","Cooling","","dBA","53","61","61","61"]
["","Heating","","dBA","53","61","61","61"]
["Dimensions","Unit","Width","mm","840","840","840","840"]
["","","Depth","mm","840","840","840","840"]
["","","Height","mm","288","288","288","288"]
["Casing","Material","","","Galvanised steel plate","Galvanised steel plate","Galvanised steel plate","Galvanised steel plate"]
["Weight","Unit","","kg","25","25","25","25"]
["Decoration panel 2","Weight","","kg","5.4","5.4","5.4","5.4"]
["","Model","","","BYCQ140D7W1W - full white","BYCQ140D7W1W - full white","BYCQ140D7W1W - full white","BYCQ140D7W1W - full white"]
["","Dimensions","Depth","mm","950","950","950","950"]
["","","Width","mm","950","950","950","950"]
["","","Height","mm","50","50","50","50"]
["","Colour","","","FRESH WHITE","FRESH WHITE","FRESH WHITE","FRESH WHITE"]
["Decoration panel 3","Dimensions","Depth","mm","950","950","950","950"]
["","","Height","mm","130","130","130","130"]
["","","Width","mm","950","950","950","950"]
["","Colour","","","FRESH WHITE","FRESH WHITE","FRESH WHITE","FRESH WHITE"]
["","Model","","","BYCQ140D7GW1 - auto cleaning panel","BYCQ140D7GW1 - auto cleaning panel","BYCQ140D7GW1 - auto cleaning panel","BYCQ140D7GW1 - auto cleaning panel"]
["","Weight","","kg","10.3","10.3","10.3","10.3"]
["Decoration panel","Weight","","kg","5.4","5.4","5.4","5.4"]
["","Model","","","BYCQ140D7W1 - white with grey louvers","BYCQ140D7W1 - white with grey louvers","BYCQ140D7W1 - white with grey louvers","BYCQ140D7W1 - white with grey louvers"]
["","Dimensions","Height","mm","50","50","50","50"]
["","","Depth","mm","950","950","950","950"]
["","","Width","mm","950","950","950","950"]
["","Colour","","","FRESH WHITE","FRESH WHITE","FRESH WHITE","FRESH WHITE"]
["Heating capacity","Total capacity","Nom.","kW","","","13.5","15.5"]
["Power supply","Phase","","","1~","1~","1~","1~"]
["","Frequency","","Hz","50/60","50/60","50/60","50/60"]
["","Voltage","","V","220-240/220","220-240/220","220-240/220","220-240/220"]
["Notes","","","","(1) - The sound power level is an absolute value indicating the power which a sound source generates.","(1) - The sound power level is an absolute value indicating the power which a sound source generates.","(1) - The sound power level is an absolute value indicating the power which a sound source generates.","(1) - The sound power level is an absolute value indicating the power which a sound source generates."]
["","","","","(2) - The BYCQ140D7W1W has white insulations. Be informed that formation of dirt on white insulation is visibly stronger and that it is consequently not advised to install the BYCQ140D7W1W decoration panel in environments exposed to concentrations of dirt.","(2) - The BYCQ140D7W1W has white insulations. Be informed that formation of dirt on white insulation is visibly stronger and that it is consequently not advised to install the BYCQ140D7W1W decoration panel in environments exposed to concentrations of dirt.","(2) - The BYCQ140D7W1W has white insulations. Be informed that formation of dirt on white insulation is visibly stronger and that it is consequently not advised to install the BYCQ140D7W1W decoration panel in environments exposed to concentrations of dirt.","(2) - The BYCQ140D7W1W has white insulations. Be informed that formation of dirt on white insulation is visibly stronger and that it is consequently not advised to install the BYCQ140D7W1W decoration panel in environments exposed to concentrations of dirt."]
["","","","","(3) - BYCQ140D7W1: pure white standard panel with grey louvers; BYCQ140D7W1W: pure white standard panel with white louvers; BYCQ140D7GW1: pure white auto cleaning panel.","(3) - BYCQ140D7W1: pure white standard panel with grey louvers; BYCQ140D7W1W: pure white standard panel with white louvers; BYCQ140D7GW1: pure white auto cleaning panel.","(3) - BYCQ140D7W1: pure white standard panel with grey louvers; BYCQ140D7W1W: pure white standard panel with white louvers; BYCQ140D7GW1: pure white auto cleaning panel.","(3) - BYCQ140D7W1: pure white standard panel with grey louvers; BYCQ140D7W1W: pure white standard panel with white louvers; BYCQ140D7GW1: pure white auto cleaning panel."]
["","","","","(4) - This option is intended exclusively for usage in fine dust environments (clothing shops). Do not use this option in high humidity and/or greasy environments.","(4) - This option is intended exclusively for usage in fine dust environments (clothing shops). Do not use this option in high humidity and/or greasy environments.","(4) - This option is intended exclusively for usage in fine dust environments (clothing shops). Do not use this option in high humidity and/or greasy environments.","(4) - This option is intended exclusively for usage in fine dust environments (clothing shops). Do not use this option in high humidity and/or greasy environments."]