{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":29,"n_cols":6,"rows_kept":29,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCQG-F / RXS-F"]
[]
[]
[]
[]
["","","","","FCQG60FVEB / RXS60F3V1B","FCQG60FVEB / RXS60F4V1B"]
["Cooling capacity","Nom.","","kW","5.70 (3)","5.70"]
["Space cooling","SEER","","","","5.74"]
["","Annual energy consumption","","kWh/a","","347"]
["","Capacity","Pdesign","kW","","5.70"]
["","Energy efficiency class","","","","A+"]
["Space heating (Average climate)","Capacity","Pdesign","kW","","4.71"]
["","SCOP/A","","","","3.87"]
["","Energy efficiency class","","","","A"]
["","Annual energy consumption","","kWh/a","","1,704"]
["Piping connections","Liquid","OD","mm","","6.35"]
["","Gas","OD","mm","","12.7"]
["","Drain","OD","mm","","VP20 (External dia.26, Internal dia. 20)"]
["Nominal efficiency","EER","","","3.48","3.48"]
["","Annual energy consumption","","kWh","820","820"]
["","COP","","","3.52","3.52"]
["","Energy labeling Directive","Cooling","","A","A"]
["","","Heating","","B","B"]
["Heating capacity","Nom.","","kW","7.00 (4)","7.00"]
["Notes","","","","(1) - Energy label: scale from A (most efficient) to G (less efficient)","(1) - EER/COP according to Eurovent 2012, for use outside EU only"]
["","","","","(2) - Annual energy consumption: based on average use of 500 running hours per year at full load (nominal conditions)","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load"]
["","","","","(3) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB; equivalent piping length: 5m; level difference: 0m"]
["","","","","(4) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m; level difference: 0m"]
["","","","","(5) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load"]