{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":7,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCQG-F / RXS-L"]
[]
[]
[]
[]
["","","","","FCQG35FVEB / RXS35L2V1B","FCQG50FVEB / RXS50L2V1B","FCQG60FVEB / RXS60L2V1B"]
["Cooling capacity","Min.","","kW","1.3","1.7","1.7"]
["","Max.","","kW","4.0","5.3","5.7"]
["","Nom.","","kW","3.4","5.0","5.7"]
["Space cooling","SEER","","","6.35","6.48","6.22"]
["","Annual energy consumption","","kWh/a","193","270","321"]
["","Capacity","Pdesign","kW","3.50","5.00","5.70"]
["","Energy efficiency class","","","A++","A++","A++"]
["Space heating (Average climate)","Capacity","Pdesign","kW","3.32","4.36","4.71"]
["","SCOP/A","","","4.90","4.29","4.00"]
["","Energy efficiency class","","","A++","A++","A+"]
["","Annual energy consumption","","kWh/a","949","1,426","1,646"]
["Piping connections","Liquid","OD","mm","6.35","6.35","6.35"]
["","Gas","OD","mm","9.5","12.70","12.70"]
["","Drain","OD","mm","VP25 (External dia.32, internal dia. 25)","VP25 (External dia.32, internal dia. 25)","VP25 (External dia.32, internal dia. 25)"]
["Nominal efficiency","Annual energy consumption","","kWh","475","705","820"]
["","EER","","","3.58","3.55","3.48"]
["","COP","","","3.50","3.7","3.52"]
["","Energy labeling Directive","Cooling","","A","A","A"]
["","","Heating","","B","A","B"]
["Heating capacity","Nom.","","kW","4.20","6.00","7.0"]
["","Min.","","kW","1.3","1.7","1.7"]
["","Max.","","kW","5.2","6.0","7.0"]
["Notes","","","","(1) - 220V","(1) - 220V","(1) - 220V"]
["","","","","(2) - 230V","(2) - 230V","(2) - 230V"]
["","","","","(3) - 240V","(3) - 240V","(3) - 240V"]
["","","","","(4) - EER/COP according to Eurovent 2012, for use outside EU only","(4) - EER/COP according to Eurovent 2012, for use outside EU only","(4) - EER/COP according to Eurovent 2012, for use outside EU only"]
["","","","","(5) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(5) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(5) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load"]