{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":16,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHA-A(9) / RZQG-L9V1"]
[]
[]
[]
[]
["","","","","FHA100AVEB / RZQG71L9V1B","FHA35AVEB9 / FHA35AVEB9 / FHA35AVEB9 / RZQG71L9V1B","FHA35AVEB9 / FHA35AVEB9 / RZQG71L9V1B","FHA50AVEB9 / FHA50AVEB9 / RZQG71L9V1B","FHA35AVEB98 / FHA35AVEB98 / FHA35AVEB98 / RZQG71L9V1B","FHA100AVEB8 / RZQG71L9V1B","FHA35AVEB98 / FHA35AVEB98 / RZQG71L9V1B","FHA50AVEB98 / FHA50AVEB98 / RZQG71L9V1B","FHA71AVEB98 / RZQG71L9V1B","FHA35AVEB99 / FHA35AVEB99 / FHA35AVEB99 / RZQG71L9V1B","FHA100AVEB9 / RZQG71L9V1B","FHA50AVEB99 / FHA50AVEB99 / RZQG71L9V1B"]
["Cooling capacity","Nom.","","kW","6.80","6.80","6.80","6.80","6.80","6.80","6.80","6.80","6.80","6.80","6.80","6.80"]
["Space cooling","SEER","","","6.86","5.10","5.10","5.10","5.10","6.86","5.10","5.10","6.86","5.10","6.86","5.10"]
["","Annual energy consumption","","kWh/a","347","467","467","467","467","347","467","467","347","467","347","467"]
["","Capacity","Pdesign","kW","6.80","6.80","6.80","6.80","6.80","6.80","6.80","6.80","6.80","6.80","6.80","6.80"]
["","Energy efficiency class","","","A++","A","A","A","A","A++","A","A","A++","A","A++","A"]
["Space heating (Average climate)","Capacity","Pdesign","kW","7.60","6.00","6.00","6.00","6.00","7.60","6.00","6.00","7.60","6.00","7.60","6.00"]
["","SCOP/A","","","4.32","3.80","3.80","3.80","3.80","4.32","3.80","3.80","4.32","3.80","4.32","3.80"]
["","Energy efficiency class","","","A+","A","A","A","A","A+","A","A","A+","A","A+","A"]
["","Annual energy consumption","","kWh/a","2,463","2,211","2,211","2,211","2,211","2,463","2,211","2,211","2,463","2,211","2,463","2,211"]
["Nominal efficiency","EER","","","3.82","3.30","3.30","3.30","3.30","3.82","3.30","3.30","3.82","3.30","3.82","3.30"]
["Notes","","","","(1) - See separate drawing for operation range","(1) - See separate drawing for operation range","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - See separate drawing for operation range","(1) - See separate drawing for operation range","(1) - See separate drawing for operation range","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - See separate drawing for operation range","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - See separate drawing for operation range","(1) - See separate drawing for operation range","(1) - See separate drawing for operation range"]
["","","","","(2) - See separate drawing for electrical data","(2) - See separate drawing for electrical data","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - See separate drawing for electrical data","(2) - See separate drawing for electrical data","(2) - See separate drawing for electrical data","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - See separate drawing for electrical data","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - See separate drawing for electrical data","(2) - See separate drawing for electrical data","(2) - See separate drawing for electrical data"]
["","","","","","","(3) - See separate drawing for operation range","","","","(3) - See separate drawing for operation range","","(3) - See separate drawing for operation range"]
["","","","","","","(4) - See separate drawing for electrical data","","","","(4) - See separate drawing for electrical data","","(4) - See separate drawing for electrical data"]
["Heating capacity","Nom.","","kW","","","","","","","","","7.50"]
["Nominal efficiency","COP","","","","","","","","","","","4.13"]
["","Annual energy consumption","","kWh","","","","","","","","","890"]
["","Energy labeling Directive","Cooling","","","","","","","","","","A"]
["","","Heating","","","","","","","","","","A"]