{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":17,"n_cols":6,"rows_kept":17,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHQ-C / RR-BV3"]
[]
[]
[]
[]
["","","","","FHQ71CAVEB / RR71B8V3B","FHQ100CAVEB / RR100B8V3B"]
["Cooling capacity","Nom.","","kW","7.1 (3)","9.8 (3)"]
["Piping connections","Liquid","OD","mm","9.52","9.52"]
["","Gas","OD","mm","15.9","15.9"]
["","Drain","OD","mm","26","26"]
["Nominal efficiency","EER","","","2.63","2.61"]
["","Annual energy consumption","","kWh","1,350","1,875"]
["","Energy labeling Directive","Cooling","","D","D"]
["Notes","","","","(1) - Annual energy consumption: based on average use of 500 running hours per year at full load (nominal conditions)","(1) - Annual energy consumption: based on average use of 500 running hours per year at full load (nominal conditions)"]
["","","","","(2) - Energy label: scale from A (most efficient) to G (less efficient)","(2) - Energy label: scale from A (most efficient) to G (less efficient)"]
["","","","","(3) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 7.5m; level difference: 0m","(3) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 7.5m; level difference: 0m"]
["","","","","(4) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(4) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load"]