{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":15,"n_cols":6,"rows_kept":15,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHQ-CB / RXS-L"]
[]
[]
[]
[]
["","","","","FHQ50CBVEB / RXS50L2V1B","FHQ60CBVEB / RXS60L2V1B"]
["Space cooling","SEER","","","5.87","6.02"]
["","Annual energy consumption","","kWh/a","298","332"]
["","Capacity","Pdesign","kW","5.00","5.70"]
["","Energy efficiency class","","","A+","A+"]
["Space heating (Average climate)","Capacity","Pdesign","kW","4.35","4.71"]
["","SCOP/A","","","3.86","3.87"]
["","Energy efficiency class","","","A","A"]
["","Pdh Heating capacity at -10°","","kW","3.85","4.08"]
["","Annual energy consumption","","kWh/a","1,578","1,705"]