{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":29,"n_cols":18,"rows_kept":29,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVA-A / RZAG-NV1"]
[]
[]
[]
[]
["","","","","FVA100AMVEB / RZAG71N7V1B","FVA100AMVEB / RZAG71N2V1B","FVA71AMVEB / RZAG71N2V1B","FVA71AMVEB / RZAG71N7V1B","FVA140AMVEB / RZAG100N2V1B","FVA140AMVEB / RZAG100N7V1B","FVA100AMVEB / RZAG100N2V1B","FVA100AMVEB / RZAG100N7V1B","FVA125AMVEB / RZAG125N2V1B","FVA125AMVEB / RZAG125N7V1B","FVA140AMVEB / RZAG140N2V1B","FVA140AMVEB / RZAG140N7V1B","FVA71AMVEB / FVA71AMVEB / RZAG140N2V1B","FVA71AMVEB / FVA71AMVEB / RZAG140N7V1B"]
["Cooling capacity","Nom.","","kW","6.80 (1)","","","","9.50 (1)","9.50 (1)"]
["Space cooling","SEER","","","6.41","","","","6.43","6.43"]
["","Annual energy consumption","","kWh/a","371","","","","517","517"]
["","Capacity","Pdesign","kW","6.80","","","","9.50","9.50"]
["","Energy efficiency class","","","A++","","","","A++","A++"]
["Space heating (Average climate)","Capacity","Pdesign","kW","4.70","","","","7.80","7.80"]
["","SCOP/A","","","4.03","","","","4.05","4.05"]
["","Energy efficiency class","","","A+","","","","A+","A+"]
["","Annual energy consumption","","kWh/a","1,634","","","","2,697","2,697"]
["Heating capacity","Nom.","","kW","7.50 (2)","","","","10.8 (2)","10.8 (2)"]
["Notes","","","","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]
["Cooling capacity","Nom.","","kW","","6.80","6.80 (1)","6.80 (1)","","","9.50 (1)","9.50 (1)","12.1 (1)","12.1 (1)","13.4 (1)","13.4 (1)","13.4 (1)","13.4 (1)"]
["Heating capacity","Nom.","","kW","","7.50","7.50 (2)","7.50 (2)","","","10.8 (2)","10.8 (2)","13.5 (2)","13.5 (2)","15.5 (2)","15.5 (2)","15.5 (2)","15.5 (2)"]
["Space cooling","Energy efficiency class","","","","A++","A++","A++","","","A++","A++"]
["","Capacity","Pdesign","kW","","6.80","6.80","6.80","","","9.50","9.50","12.1","12.1","13.4","13.4","13.4","13.4"]
["","SEER","","","","6.41","6.34","6.34","","","6.40","6.40","6.41","6.41","6.12","6.12","8.31","8.31"]
["","Annual energy consumption","","kWh/a","","371","376","376","","","520","520","1133","1133","1314","1314","968","968"]
["Space heating (Average climate)","Energy efficiency class","","","","A+","A+","A+","","","A+","A+"]
["","Capacity","Pdesign","kW","","4.70","4.70","4.70","","","7.80","7.80","9.52","9.52","9.52","9.52","9.52","9.52"]
["","SCOP/A","","","","4.03","4.05","4.05","","","4.20","4.20","4.15","4.15","3.94","3.94","4.37","4.37"]
["","Annual energy consumption","","kWh/a","","1634","1625","1625","","","2600","2600","3209","3209","3383","3383","3050","3050"]
["Energy Efficiency Range","","","","","","A+++ ~ D","A+++ ~ D","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D"]